Neptune4

LED修正メモ

1.Add these to your printers home/mks folder. Open Putty and run bash install.sh (Its normal if it returns an oooopsie,just move on) Remove lines in printer.cfg about flashlight and replace with these: [gcode_shell_command hotend] command: sh /home/mks/toggleled.sh timeout: 30. verbose: True

[gcode_shell_command overhead] command: sh /home/mks/toggleovr.sh timeout: 30. verbose: True

[gcode_macro Hotend LED] description: Turn on Hotend LEDs gcode:

RUN_SHELL_COMMAND CMD=hotend

[gcode_macro Overhead LED] description: Turn on Hotend LEDs gcode:

RUN_SHELL_COMMAND CMD=overhead

4: Profit